Tender specifications: Portal CB 10

High quality, especially wear-resistant entrance mat, improved absorption of coarse dirt

Application: Indoor and roofed exterior; normal up to extremely strong frequency, suitable for trolley and wheelchairs, overall laying, Static point loading up to 5000 kg per 80 cm²

Stripe profile: aluminum, with scratching edge, sound insulated

Cassette brush: with bristle bundles arranged parallel to one another, colour black, slip resistance R 12 according to DIN 51130

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections -, each part can easily be replaced on the spot

Height: 10 mm

Bar distance: 5 or 7 mm

(\_) 5 mm

(\_) 7 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Portal CB 10

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de