Tender specifications: Portal GB 17 Mix 2/1

High quality, especially wear-resistant entrance mat, improved absorption of coarse dirt

Application: Indoor and exterior; normal up to extremely strong frequency, suitable for trolleys and wheelchairs, overall laying, resting distributed burden up to 3000 kg per 80 cm²

Stripe profile: aluminum, with scratching edge, sound insulated

Cleaning stripes: Rubber and brush, mix 2/1 (minimum 32 brush profiles each metre of walking depth)

Rubber profiles: serrated lengthways; aluminum profile edges covered, high quality material mix, colour black; slip resistance R 9 according to DIN 51130

Brush: ARWEI three-way brush; brushes on different levels for an improved absorption of coarse dirt, sound insulating, colour black, slip resistance R 13 according to DIN 51130

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections-, each part can easily be replaced on the spot

Height: 17 mm

Bar distance 4 mm: 33 brush profiles each m of walking depth

Bar distance 6 mm: 32 brush profiles each m of walking depth

Angle frames in 20 x 20 x 3 mm are available in aluminum, brass or stainless steel.

(\_) 4 mm

(\_) 6 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Portal GB 17 Mix 2/1

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de