Tender specifications: Portal GEK 17

High quality, especially wear-resistant entrance mat, improved absorption of coarse dirt

Application: Indoor and roofed exterior; normal up to extremely strong frequency, suitable for trolley and wheelchairs, overall laying, Static point loading up to 2900 kg per 80 cm²

Stripe profile: aluminum, with sideways integrated scratching edges put inbetween the profiles, sound insulated

Cleaning stripes: Rubber and single scratching edge alternating

Rubber profiles: serrated lengthways; high quality material mix, colour black; slip resistance R 9 according to DIN 51130

Single scratching edge: put inbetween the rubber profiles, high quality material mix, flexible, thus gentle to shoes; no aluminum reflection

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections-, each part can easily be replaced on the spot

Height: 17 mm  
Bar distance: 4 or 6 mm  
At a bar distance of 4 mm also appropriate for automatically revolving doors according to DIN 18650-1.  
Angle frames in 20 x 20 x 3 mm are available in aluminum, brass or stainless steel.

(\_) 4 mm

(\_) 6 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Portal GEK 17

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de