Tender specifications: Portal SN 12

High quality, especially wear-resistant entrance mat

Application: Indoor and roofed exterior; normal up to extremely strong frequency, drivable for trolleys, pallet trucks, cars, etc.; suitable for wheelchairs, overall laying, Static point loading up to 6500 kg per 80 cm²

Stripe profile: aluminum, with scratching edge, sound insulated

Nadelvliessonderboden: vollflächig vernadelt; keine Schlingenware; minimale Anschmutzung; extrem abriebfest;

verdeckt liegend gegen seitliches Verrutschen gesichert; Nadelvlies nachträglich austauschbar;

Rutschhemmung R 11 nach DIN 51130

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections -, each part can easily be replaced on the spot

Height: 12 mm

Bar distance: 4 or 6 mm

(\_) 4 mm

(\_) 6 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Portal SN 12

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de