Tender specifications: Tradition RCB 22

High quality, especially wear-resistant entrance mat, improved absorption of coarse dirt

Application: Indoor and roofed exterior; normal up to extremely strong frequency, suitable for trolley and wheelchairs, overall laying, Static point loading up to 1200 kg per 80 cm²

Stripe supporting profile: aluminum, V-shaped; 3 mm ground clearance, uncoupled, sound-absorbing, rinsing, rear ventilated

Cleaning stripes: Rips and cassette brush alternating

Walking area: Rips, 100 % PP; is fixed in a covered manner to prevent slipping sideways; can be substituted subsequently; colours anthracite, light grey, dark brown, red, coconut; slip resistance R11 according to DIN 51130

Cassette brush: with bristle bundles arranged parallel to one another, colour black, slip resistance R 12 according to DIN 51130

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections -, each part can easily be replaced on the spot

Height: 22 mm

Bar distance 3 mm: Coarse dirt absorption 7,7 l / m²

Bar distance 5 mm: Coarse dirt absorption 8,6 l / m²

Angle frames in 25 x 25 x 3 mm are available in aluminum, brass or stainless steel.

(\_) 3 mm

(\_) 5 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Tradition RCB 22

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de